IP (tos 0xc0, ttl 1, id 4052, offset 0, flags [none], proto OSPF (89), length 172)
    40.35.1.2 > 224.0.0.5: OSPFv2, LS-Update, length 152
	Router-ID 10.255.245.35, Backbone Area, Authentication Type: none (0), 1 LSA
	  LSA #1
	  Advertising Router 10.255.245.37, seq 0x80000002, age 9s, length 104
	    Area Local Opaque LSA (10), Opaque-Type Traffic Engineering LSA (1), Opaque-ID 8
	    Options: [External]
	    Link TLV (2), length: 100
	      Link Type subTLV (1), length: 1, Point-to-point (1)
	      Link ID subTLV (2), length: 4, 10.255.245.69 (0x0afff545)
	      Local Interface IP address subTLV (3), length: 4, 10.9.142.1
	      Remote Interface IP address subTLV (4), length: 4, 10.9.142.2
	      Traffic Engineering Metric subTLV (5), length: 4, Metric 63
	      Maximum Bandwidth subTLV (6), length: 4, 622.080 Mbps
	      Maximum Reservable Bandwidth subTLV (7), length: 4, 622.080 Mbps
	      Unreserved Bandwidth subTLV (8), length: 32
		TE-Class 0: 622.080 Mbps
		TE-Class 1: 622.080 Mbps
		TE-Class 2: 622.080 Mbps
		TE-Class 3: 622.080 Mbps
		TE-Class 4: 622.080 Mbps
		TE-Class 5: 622.080 Mbps
		TE-Class 6: 622.080 Mbps
		TE-Class 7: 622.080 Mbps
	      Administrative Group subTLV (9), length: 4, 0x00000000
IP (tos 0xc0, ttl 1, id 4106, offset 0, flags [none], proto OSPF (89), length 172)
    40.35.1.2 > 224.0.0.5: OSPFv2, LS-Update, length 152
	Router-ID 10.255.245.35, Backbone Area, Authentication Type: none (0), 1 LSA
	  LSA #1
	  Advertising Router 10.255.245.37, seq 0x80000002, age 9s, length 104
	    Area Local Opaque LSA (10), Opaque-Type Traffic Engineering LSA (1), Opaque-ID 9
	    Options: [External]
	    Link TLV (2), length: 100
	      Link Type subTLV (1), length: 1, Point-to-point (1)
	      Link ID subTLV (2), length: 4, 10.255.245.69 (0x0afff545)
	      Local Interface IP address subTLV (3), length: 4, 10.9.143.1
	      Remote Interface IP address subTLV (4), length: 4, 10.9.143.2
	      Traffic Engineering Metric subTLV (5), length: 4, Metric 63
	      Maximum Bandwidth subTLV (6), length: 4, 622.080 Mbps
	      Maximum Reservable Bandwidth subTLV (7), length: 4, 622.080 Mbps
	      Unreserved Bandwidth subTLV (8), length: 32
		TE-Class 0: 622.080 Mbps
		TE-Class 1: 622.080 Mbps
		TE-Class 2: 622.080 Mbps
		TE-Class 3: 622.080 Mbps
		TE-Class 4: 622.080 Mbps
		TE-Class 5: 622.080 Mbps
		TE-Class 6: 622.080 Mbps
		TE-Class 7: 622.080 Mbps
	      Administrative Group subTLV (9), length: 4, 0x00000000
IP (tos 0xc0, ttl 1, id 4160, offset 0, flags [none], proto OSPF (89), length 212)
    40.35.1.2 > 224.0.0.5: OSPFv2, LS-Update, length 192
	Router-ID 10.255.245.35, Backbone Area, Authentication Type: none (0), 1 LSA
	  LSA #1
	  Advertising Router 10.255.245.35, seq 0x80000003, age 3s, length 144
	    Area Local Opaque LSA (10), Opaque-Type Traffic Engineering LSA (1), Opaque-ID 3
	    Options: [External]
	    Link TLV (2), length: 140
	      Link Type subTLV (1), length: 1, Point-to-point (1)
	      Link ID subTLV (2), length: 4, 10.255.245.40 (0x0afff528)
	      Local Interface IP address subTLV (3), length: 4, 10.40.35.14
	      Remote Interface IP address subTLV (4), length: 4, 10.40.35.13
	      Traffic Engineering Metric subTLV (5), length: 4, Metric 1
	      Maximum Bandwidth subTLV (6), length: 4, 100.000 Mbps
	      Maximum Reservable Bandwidth subTLV (7), length: 4, 100.000 Mbps
	      Unreserved Bandwidth subTLV (8), length: 32
		TE-Class 0: 0.000 Mbps
		TE-Class 1: 0.000 Mbps
		TE-Class 2: 0.000 Mbps
		TE-Class 3: 0.000 Mbps
		TE-Class 4: 0.000 Mbps
		TE-Class 5: 0.000 Mbps
		TE-Class 6: 0.000 Mbps
		TE-Class 7: 0.000 Mbps
	      Interface Switching Capability subTLV (15), length: 44
		Interface Switching Capability: Packet-Switch Capable-1
		LSP Encoding: Ethernet V2/DIX
		Max LSP Bandwidth:
		  priority level 0: 0.000 Mbps
		  priority level 1: 0.000 Mbps
		  priority level 2: 0.000 Mbps
		  priority level 3: 0.000 Mbps
		  priority level 4: 0.000 Mbps
		  priority level 5: 0.000 Mbps
		  priority level 6: 0.000 Mbps
		  priority level 7: 0.000 Mbps
